**AP7.30. APPENDIX 7.30**

**HAZARDOUS WASTE/MATERIAL CODE**

|  |  |  |
| --- | --- | --- |
| NUMBER OF CHARACTERS: | | One (Generator Communication Legacy)/Two (DLMS) |
| TYPE OF CODE: | | Alpha |
| EXPLANATION: | | Entered on the DTID Record supporting a Hazardous Material/Hazardous Waste Turn-In to DLA Disposition Services to identify the nature of the hazard and service request. The Generator Communication (GenComm) legacy format is one alpha character. Under the DLMS, this value is converted to a two position alpha character for alignment with the Disposition Services Indicator DLMS data element. |
| RECORD POSITION(S): | | GENCOMM DTID Record Format (8th data element) |
| DLMS SEGMENT/QUALFIER | | LQ Segment, LQ01 Data Element ID 1270 Qualifier “DSI – Disposition Services Indicator” |
|  | |  |
| CODE | EXPLANATION | |
| HM | Hazardous Material. GenComm legacy equivalent code is M. | |
| HW | Hazardous and Non-Regulated Waste. GenComm legacy equivalent code is W. | |
| SC | Scrap Property. GenComm legacy equivalent code is S. | |
| SS | Special Services Request. GenComm legacy equivalent code is P. | |
| US | Useable Property. GenComm legacy equivalent code is N. | |